**Proper Care and Maintenance of Stage Curtains**

Stage Curtains properly care for should last 20-30 years or longer. Misused and not cared for stage curtains will need to be replaced in just years.

**Proper Care of a Curtain includes:**

1. **Vacuuming**. Once a year the curtain should be vacuumed completely. Dust is the enemy of stage curtains. The dust accumulates, leaches the fire retardency out of the curtain and causes it to dry rot. Vacuum each year.
2. **Cleaning**. The curtain should be professionally cleaned every 7 years if vacuumed yearly or every three to five years if not vacuumed annually. This deep cleaning is critical to a curtain’s long life
3. **Repairs.** Because LuXout is one of the major replacement stage curtain manufacturers in the country we do our own repairs to maximize the longevity of your curtains.
4. **Environmental Control.** Stage Curtains need to be maintained in a controlled area. Too much humidity and the curtains can shrink, ruin flame retardency and dry rot.

**LuXout Curtain Maintenance Services**

* Repair of snag and tears
* Cleaning
* Fire retardency treatment
* Replacement Curtains
* Replacement Track
* Curtain Motorization

**Other LuXout Products and Services**

* Theatre Window treatment Cleaning
* Window treatment fire retardant treatment
* Window treatment repairs
* New Window Treatments
* Automated window treatments

**LuXout Services**

* Available in Virginia, Maryland, North Carolina, DC and Florida directly from our field service staff for take down, re-hang and services above
* Outside of areas above Services through our network of dealers and agents across the country. Call us at 800-817-1204.
* Outside our direct service areas dealers can assist you in taking down your curtains, shipping them to our cleaning plant and re-hanging them for you when ready. A complete turnkey solution to your needs.